//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Button PLLBYPASS1 // SET HIGH 
//Button PLLBYPASS0 // SET LOW 
//Button PLLSEL1  // SET HIGH 
//Button PLLSEL0  // SET LOW 
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 


.Set READY_VAR = 01

Command ID:	PROTOCOL_OPTION  
Send	Command: 84 A9 61 00 02 00 55 80
Receive	Data:84 A9 61 00 02 00 55 00
Command ID: DPMR_M_F
Send command: 84 A9 61 00 02 03 54 1a
Receive Data: 84 A9 61 00 02 03 54 00
Command ID: DPMR_SLD
Send command: 84 A9 61 00 06 03 56 11 22 c4 48 bf 
Receive Data: 84 A9 61 00 02 03 56 00
Command ID: DPMR_HT_CI
Send command: 84 A9 61 00 03 03 57 F0 00
Receive Data: 84 A9 61 00 02 03 57 00
Command ID: DPMR_END_UE
Send command: 84 A9 61 00 04 03 4B 1f 00 00
Receive Data: 84 A9 61 00 02 03 4B 00
Command ID:	ADDRESSING_MODE
Send	Command: 84 A9 61 00 02 03 28 01
Receive	Command:84 A9 61 00 02 03 28 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 12 34 56
Receive Data: 84 A9 61 00 02 03 50 00
Command ID: DPMR_OWN_ID_BCD
Send command: 84 A9 61 00 05 03 53 11 22 33 44
Receive Data: 84 A9 61 00 02 03 53 00
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 03
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID: REPORT_FIELD
Send command: 84 A9 61 00 02 00 1D 74
Receive Data: 84 A9 61 00 02 00 1D 00
Command ID: WORK_MODE_DUPLEX
Send command: 84 A9 61 00 04 00 18 03 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: CARRIER_READY&CALL_START
Send command: 84 A9 61 00 04 00 20 1a 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Receive Data: 84 A9 61 00 04 30 51 19 11 66
Receive Data:84 A9 61 00 02 30 27 05
PAUSE 1000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 1F 00 00
PAUSE 1000
Command ID: CARRIER_LOSE
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 01
Receive	Data:84 A9 61 00 02 00 10 00
pause 2000
Command ID: CARRIER_READY&CALL_START
Send command: 84 A9 61 00 04 00 20 1a 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Receive Data: 84 A9 61 00 04 30 51 19 11 66
Receive Data:84 A9 61 00 02 30 27 05
PAUSE 1000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 1F 00 00
PAUSE 1000
Command ID: CARRIER_LOSE
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 ff
Receive	Data:84 A9 61 00 02 00 10 00
pause 100
Command ID: CARRIER_READY&CALL_START
Send command: 84 A9 61 00 04 00 20 1a 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Receive Data: 84 A9 61 00 04 30 51 19 11 66
Receive Data:84 A9 61 00 02 30 27 05
PAUSE 2000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 1F 00 00
PAUSE 1000
Command ID: CARRIER_LOSE
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Command ID: CARRIER_READY&CALL_START
Send command: 84 A9 61 00 04 00 20 1a 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Receive Data: 84 A9 61 00 04 30 51 19 11 66
Receive Data:84 A9 61 00 02 30 27 05
PAUSE 1000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 1F 00 00
PAUSE 1000
Command ID: CARRIER_LOSE
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Command ID: CARRIER_READY&CALL_START
Send command: 84 A9 61 00 04 00 20 0a 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 0a
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Receive Data: 84 A9 61 00 04 30 51 19 11 66
Receive Data:84 A9 61 00 02 30 27 05
PAUSE 2000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 1F 00 00
PAUSE 1000
Command ID: CARRIER_LOSE
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Command ID: CARRIER_READY&CALL_START
Send command: 84 A9 61 00 04 00 20 0a 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 0a
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Receive Data: 84 A9 61 00 04 30 51 19 11 66
Receive Data:84 A9 61 00 02 30 27 05
PAUSE 1000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 1F 00 00
PAUSE 1000
Command ID: CARRIER_LOSE
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 03
Receive	Data:84 A9 61 00 02 00 10 00
pause 2000
Command ID: CARRIER_READY&CALL_START
Send command: 84 A9 61 00 04 00 20 1a 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Receive Data: 84 A9 61 00 04 30 51 19 11 66
Receive Data:84 A9 61 00 02 30 27 05
PAUSE 2000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 1F 00 00
PAUSE 1000
Command ID: CARRIER_LOSE
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00

