Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
.Set READY_VAR = 01
//Command ID:	DMR_CC
//Send	Command: 84 A9 61 00 02 05 77 0d
//Receive	Data:84 A9 61 00 02 05 77 00
Command ID:	PROTOCOL_OPTION
Send	Command: 84 A9 61 00 02 00 55 80
Receive	Data:84 A9 61 00 02 00 55 00
Command ID:	NXDN_SR
Send	Command: 84 A9 61 00 02 06 77 01
Receive Data:   84 A9 61 00 02 06 77 00 
Command ID:	WORK_MODE_RX
Send	Command: 84 A9 61 00 04 00 18 01 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 83
Receive	Data:84 A9 61 00 02 00 1A 00
Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 84 01
Receive	Command:84 A9 61 00 02 00 26 00
//Command ID:	DMR_CALL_OPTION for 3918 controlled RF
//Send	Command: 84 A9 61 00 06 05 79 c1 00 00 00 00 
//Command ID:	DMR_CALL_OPTION
//Send	Command: 84 A9 61 00 06 05 79 c1 00 00 00 00 
//Receive	Data:84 A9 61 00 02 05 79 00
Command ID:	NXDN_CALL_OPTION
Send	Command: 84 A9 61 00 06 06 47 82 00 00 00 00
Receive Data:   84 A9 61 00 02 06 47 00
Pause 1000
Command ID:	DEMOD_GAIN
Send	Command: 84 A9 61 00 03 00 1C 00 00
Receive	Command:84 A9 61 00 02 00 1C 00
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 2000
